Installation for WindowsXP SP2 and Cybermouse 30S. (11.4.2005)

This driver installation is intended for using PC/SC driver for the serial
Cybermouse 30S within Microsoft WindowsXP and service pack 2. It should also
works with Cybermouse 20S but has not been tested roughly. Furthermore support
for Cybermouse 20S might be canceled in further releases.

Prior to installation please remove all previous installed Cybermouse drivers.

For installation please follow these steps:
- plug in Cybermouse 30S into serial port and keybord/mouse PS/2 port.
- run the setup.exe program
- step forward through the installation dialogs.
- after the 'finish' dialog the installation will start.
- there are several system dialogs security warnings about uncertified drivers.
  Please continue the installation.
- After installation a second driver will be installed. This will be done
  automatically through the system "Found New Hardware Wizard".
  You will be prompt "Can Windows connect to Windows Update to search for
  software?" but you should select the 3rd selection ("No, not this time").
  Please proceed (Press button "Next>").
  Next dialog you will be prompt "What do you want the wizard to do?". Please
  select the first selection ("Install the software automatically
  (Recommended)" and proceed (Press button "Next>").
  In the 3rd dialog please press button "finish".
  Now wait until system prompt for an successfully installed driver.

Limitations:
- it might be necessary to reboot after installation.
- presence of Cybermouse is only detected during startup.  
- only the CyberMouse connected to the first two system ports are
  detected/supported


# :vi:set expandtab
